|  |  |  |  |
| --- | --- | --- | --- |
| **·Huawei Technologies Co., Ltd.** | Document No. | Product Version | Confidential Level |
|  | V200R001 | Internal Open |
| Product Name：E5170s-22 | | Total 6 pages |

Local Web-upgrade Guide for E5170s-22

（Internal Open）

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Athour： | m00206464 |  | Date： | 2013-09-25 |
| Assessor： |  |  | Date： |  |
| Approver： |  |  | Date： |  |



**HUAWEI TECHNOLOGIES CO., LTD.**

Copyright © Huawei Technologies Co., Ltd. 2010. All rights reserved.

Contents

[1 Overview 3](#_Toc367889154)

[1.1 Upgrade Instruction 3](#_Toc367889155)

[1.2 Nomenclature 3](#_Toc367889156)

[2 Pre-upgrade Checklist 3](#_Toc367889157)

[2.1 Obtaining Upgrade Script Package and Tools 3](#_Toc367889158)

[2.2 Database Tables 3](#_Toc367889159)

[3 Performing the E5170’s Local Web-upgrade 3](#_Toc367889160)

[3.1 Pre-upgrade work 3](#_Toc367889161)

[3.1.1 Operating System\Database Configuration Files\Kernel Parameter\ Running Status 3](#_Toc367889162)

[3.2 Performing the Upgrade and Verifying the Result 3](#_Toc367889163)

[3.2.1 Verifying the Final Result of Upgrade 6](#_Toc367889164)

# Overview

## Upgrade Instruction

This document describes how to carry out the upgrade for E5170 of V200R001 version with the Web UI.

## Nomenclature

NA.

# Pre-upgrade Checklist

## Obtaining Upgrade Script Package and Tools

|  |  |
| --- | --- |
| **文件** | **描述** |
| B710C0UPDATE\_21.236.11.00.00.gz.bin | E5170 upgrade script package. The first characters of package name are B710C0UPDATE which are generated according to MBB’s criterion of product name. The follow-up parts are decided by pack-making method. |

**Table 1 Upgrade files**

## Database Tables

NA.

# Performing the E5170’s Local Web-upgrade

## Pre-upgrade work

Operating System\Database Configuration Files\Kernel Parameter\ Running Status

It could be used on Windows XP/Vista/Win7（Chinese or English）operating system.


## Performing the Upgrade and Verifying the Result

1. Please open the browser and input 192.168.1.1(gateway address) in the URL frame( The IP address may be different in the custom version. However, we can get it from the PC’s local connection which is connected with the E5170 and can show the specific gateway address). Then we get the login page of the E5170.



**Figure 1** Login page


1. After inputing the user name and password, click the button ‘Login’. Then click the label ‘Update → Update Manually’, and enter the page of local upgrade.



**Figure 2** Upgrade page


1. Click the button ‘browse’ to choose the correct upgrade file. Then click ‘Update’
2. Begin to upload the file to E5170. Pleaes wait a moment.

**Attention: Don’t turn off the power or remove the netting twines during uploading the file in order to avoid abnormity.**



**Figure 3** Uploading the file

1. Upgrading successfully.



**Figure 4** Upgrading successfully

1. Restarting successfully and the upgrade is completely. Click ‘here’ to login page.



**Figure 5** Refresh the page to log in after update succeeded

Verifying the Final Result of Upgrade



Attention：Don’t make the E5170 interruption of power supply during the upgrade.

|  |  |
| --- | --- |
| **Final Result** | **Guage Bar Showing** |
| Upgrading successfully | **Update succeeded.** |
| Failing to update | **Update failed.** |

**Table 2** The final show of guage bar during the upgrade( abnormity included)