**MF915**

**BD\_TMOMF915V5.0**

**Release Notes**

**Sept 2, 2014**

**ZTE® Proprietary**

**Restricted Distribution:** This document contains critical information about ZTE products and may not be distributed to anyone else without the approval from ZTE.

All data and information contained in or disclosed by this document is confidential and proprietary information of ZTE. ZTE is a registered trademark and registered service mark of ZTE Corporation.

ZTE Corporation

Address: ZTE Plaza, Keji Road South, Hi-tech Industrial Park, Nan Shan District, Shenzhen, P.R.China, 518057

© 2010 ZTE Corporation. All rights reserved.Contents

[1 Version Information 3](#_Toc393375515)

[2 Revision History 3](#_Toc393375516)

[3 Implemented requirement 3](#_Toc393375517)

[4 Fixed QC Issues 4](#_Toc393375518)

[5 Fixed internal issues 4](#_Toc393375519)

[6 Known Issues 5](#_Toc393375520)

[7 Qualcomm CR 5](#_Toc393375521)

# 1 Version Information

|  |  |
| --- | --- |
| Model Name | MF915 |
| Firmware | BD\_TMOMF915V5.0 |
| Drivers version | NO |
| Supplier | ZTE |
| Hardware version | xw5A |

# 2 Revision History

The revision history for software:

|  |  |  |
| --- | --- | --- |
| **Doc number** | **Date** | Description |
| 1 | 2014-7-2 | BD\_TMOMF915V1.0 |
| 2 | 2014-7-10 | BD\_TMOMF915V1.1 |
| 3 | 2014-7-17 | BD\_TMOMF915V2.0 |
| 4 | 2014-7-24 | BD\_TMOMF915V3.0 |
| 5 | 2014-8-7 | BD\_TMOMF915V3.1 |
| 6 | 2014-8-13 | BD\_TMOMF915V3.2 |
| 7 | 2014-8-26 | BD\_TMOMF915V4.0 |
| 8 | 2014-9-2 | BD\_TMOMF915V5.0 |
|  |  |  |

# 3 Implemented requirement

**BD\_TMOMF915V1.0：**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Num.** | **Ver.** | **PRI** | **Description** | **OS** | **Comments** |
| 1 |  |  | TMO Requirements：  (1)display wifi password on the device-ui default  (2)Display the time in AM/PM format |  |  |

# 4 Fixed QC Issues

|  |  |  |  |
| --- | --- | --- | --- |
| **Defect ID** | **Function** | **Issue Description** | **Comments/Solutions** |
| 52782 | Generic Application | “You have login through Device UI” Alert message | Fixed in V4.0 |
| 52886 |  | 'FUT:Debels William: Login scenarios | Fixed in V4.0 |
| 52888 |  | 'FUT:Debels Williams:Entering wrong password in web UI | Fixed in V4.0 |
| 52882 | UI | UI: Number of Connections not accurate | Fixed in V4.0 |
| 52785 | UI | FUT:Jennifer Greene:Set up/Not showing connection | Fixed in V4.0 |
| 52824 | UI | FUT:Quintana, Cecil: Incorrect time | Fixed in V4.0 |
| 52886 | Data performance | UMTS data performance report: UL through puts | Fixed in V4.0 |

# 5 Fixed internal issues

**BD\_TMOMF915V1.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | Lack of the words ‘http://’for the URL displayed on the device-ui |  |
| 2 | Device-UI | Upgrade detection can be execut while disconnect the network. |  |
| 3 | Device-UI | The screen can’t light off in the menu of input pin code. |  |
| 4 | WEB-UI | Device-ui can’t operate when opened the web-ui before plug the USB cable. |  |
|  |  |  |  |

**BD\_TMOMF915V1.1：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | WEB-UI | When don’t insert sim-card,the web-ui pin menu will notify ‘Pin code already locked,please contact with operator’ |  |
| 2 | WIFI | The wifi number will increase 1 after wifi-client connected fail. |  |

**BD\_TMOMF915V2.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | WEB-UI | Cann’t input ‘ ’or ‘-’in the middle location of WPS pin code. |  |
| 2 | WEB-UI | Web interface -> SMS -> Click on an SMS -> Delete  Result: A message appears on the screen which says "Are you sure to delete?". It should be "Are you sure you want to delete the text?" |  |
| 3 | Device-UI | Device-ui displayed ‘PIN Unblock Code’instead of ‘PIN unblock code’. |  |
| 4 | FUT-0012 | When looking at Device Info, the 12 digit serial number, but then displays random gibberish after it after changing the SSID. Resetting it with the reset button (under the SIM cover) returns the settings back to stock setup with a normal looking serial number, but after changing the SSID again, it appends a gibberish character or two. |  |

**BD\_TMOMF915V3.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | FUT-0010 | I went to turn on the device and it quickly turned on and then off. |  |
| 2 | FUT-0019 | Time does not update on the device screen |  |

**BD\_TMOMF915V3.1：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | FUT-0024 | 【FUT】【Button】Button Sensitivity |  |
| 3 | FUT-0004 | 【FUT】【web ui】Battery Indicator Shows Charging on WebUI |  |

**BD\_TMOMF915V3.2：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Power on | The device ui will display ‘Goodbye’ when power on if plug out USB cable before the power off process finished.. |  |

**BD\_TMOMF915V5.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | The number of wifi client isn’t accurate |  |

# 6 Known Issues

None

# 7 Qualcomm CR

None