**MF64**

**BD\_TMOMF64V3.0**

**Release Notes**

**July 24, 2014**

**ZTE® Proprietary**

**Restricted Distribution:** This document contains critical information about ZTE products and may not be distributed to anyone else without the approval from ZTE.

All data and information contained in or disclosed by this document is confidential and proprietary information of ZTE. ZTE is a registered trademark and registered service mark of ZTE Corporation.

ZTE Corporation

Address: ZTE Plaza, Keji Road South, Hi-tech Industrial Park, Nan Shan District, Shenzhen, P.R.China, 518057

© 2010 ZTE Corporation. All rights reserved.Contents

[1 Version Information 3](#_Toc392517024)

[2 Revision History 3](#_Toc392517025)

[3 Implemented requirement 3](#_Toc392517026)

[4 Fixed QC Issues 4](#_Toc392517027)

[5 Fixed internal issues 4](#_Toc392517028)

[6 Known Issues 6](#_Toc392517029)

[7 Qualcomm CR 6](#_Toc392517030)

# 1 Version Information

|  |  |
| --- | --- |
| Model Name | MF64 |
| Firmware | BD\_TMOMF64V3.0 |
| Drivers version | No driver |
| Supplier | ZTE |
| Hardware version | dfdB |

# 2 Revision History

The revision history for software:

|  |  |  |
| --- | --- | --- |
| **Doc number** | **Date** | Description |
| 1 | 2014-5-21 | BD\_TMOMF64V1.0 |
| 2 | 2014-6-5 | BD\_TMOMF64V1.1 |
| 3 | 2014-6-12 | BD\_TMOMF64V1.2 |
| 4 | 2014-6-21 | BD\_TMOMF64V1.3 |
| 5 | 2014-7-3 | BD\_TMOMF64V2.0 |
| 6 | 2014-7-16 | BD\_TMOMF64V2.1 |
| 7 | 2014-7-24 | BD\_TMOMF64V3.0 |
|  |  |  |
|  |  |  |

# 3 Implemented requirement

**BD\_TMOMF64V1.0:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Num.** | **Ver.** | **PRI** | **Description** | **Comments** |
| 1 |  |  | TMO Requirements:  (1)Config the settings of device-ui wifi password display in the web-ui.  (2)PST time display on the device-ui  (3)Device-UI and WEB-UI modified the display wording after 3 times PIN code input wrong. | Implemented |

# 4 Fixed QC Issues

|  |  |  |  |
| --- | --- | --- | --- |
| **Defect ID** | **Function** | **Issue Description** | **Comments/Solutions** |
| 52588 | Signal bar display during data usage and idle state | During active data usage, DUT displays 4G but it reverts back to 3G at Idle sate.  thus 4G is only displayed only when the devic is ondedicated state. | Fixed in V3.0 |
| 52589 | Display time | DUT is displaying Military time as default, is this the agreed standard with TMO | Fixed in V2.1 |

# 5 Fixed internal issues

**BD\_TMOMF64V1.0:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | The wording of length more than 12 can’t roll in the device-UI | Fixed |
| 2 | Device-UI | The time displayed on the device isn’t match the PST summer time of America | Fixed |
| 3 | Device-UI | Modified the power off charging cartoon image to bigger | Fixed |
| 4 | Device-UI | There is no cartoon displayed when low power off | Fixed |
| 5 | WEB-UI | The setting of button to modify the SSID or wifi distance can’t click. | Fixed |

**BD\_TMOMF64V1.1:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | While config the wifi to any kinds encrypt type , the oled display WPA2 encrypt type password all time. | Fixed |
| 2 | Device-UI | The OLED will blink when double click WPS key | Fixed |
| 3 | Device-UI | The device-ui should be display ‘PIN Lock’ when the SIM card enabled | Fixed |
| 4 | Device-UI | The time of minutes should be display as ’16:09’,while the format is 16:9 | Fixed |
| 5 | Device-UI | The default setting of data volume is 5GB while user don’t config it by the web-ui. | Fixed |

**BD\_TMOMF64V1.2:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | Display the wrong code when can’t connect network | Fixed |

**BD\_TMOMF64V1.3:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | Device-UI | When the time display at PM time,the oled will display AM one time if user push the wps button at same time. | Fixed |
| 2 | WEB-UI | Add one URL to query the data amounts buyed by user. | Fixed |
| 3 | WEB-UI | Modified some words according to operator’s suggestion | Fixed |

**BD\_TMOMF64V2.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | password | FUT-BUG-0001:  it might just be i missed something but i cant find were to find the password for this thing when i log it in | Fixed |
| 2 | Time  display | FUT-BUG-0003:  The time on the device display appears to be Pacific and I'm on Central time. I've looked through the web interface but can't find a setting to change the time zone. | Fixed |
| 3 | Constantly switching 2G/3G/4G | FUT-BUG-0004:  The device constantly switches between 2G, 3G, and 4G. The device remains stationary, close to a window. I compared this to my T-Mobile cell phone and my T-Mobile cell phone has a strong 4G, not LTE, signal. | Fixed |
| 4 | WEB-UI | Display the time on the AM or PM format | Fixed |
| 5 | Device-UI | Enable the password in default | Fixed |
| 6 | Device-UI | Display the ‘\*’ long as the length of password | Fixed |

**BD\_TMOMF64V2.1：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | WEB-UI | Web interface -> SMS -> Click on an SMS -> Delete  Result: A message appears on the screen which says "Are you sure to delete?". It should be "Are you sure you want to delete the text?" or just "Are | Fixed |
| 2 | Device-UI | Look at the time when it would show 12:08 PM. It is showing 00:08 PM, which is not a time here in the U.S. It is using European 24 hour time instead of AM/PM. | Fixed |

**BD\_TMOMF64V3.0：**

|  |  |  |  |
| --- | --- | --- | --- |
| **Issue** | **Function** | **Issue Description** | **Comments/Solutions** |
| 1 | SMS | Didn’t delete SMS when restore factory setting | Fixed |

# 6 Known Issues

None

# 7 Qualcomm CR

None